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	Table 1
1.12
	te
	The properties of the weld toe are essential for the quality and fatigue life of the welded component. In laser beam arc hybrid welding the chance to obtain good quality in the weld toe in as welded condition is also higher which should benefit the process if regarded in this standard.
	Keep limits for incorrect weld toe regarding weld toe angle, and amend limits for weld toe radius.
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